

***Check Weigher TOPY-100/1200/3000g***



Applied to automatic online package weighing and sorting. Auto-Statistic function turn weighing, maintenance, operation, statistic to more easier.

**Features**

* Strong stainless steel structure; Water proof design.
* High accurate load cell; Based on advanced DSP technology.
* Automatic weighing compensation and zero tracking.
* 100 products preset; Easy to edit and recall.
* Quickly product shift and speed recall.
* 2000 sorting records; Printer output ready.
* LCD with Touch screen; Friendly operation interface.

**Parameter**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **TOPY-100g** | **TOPY-1200g** | **TOPY-3000g** |
| Measurement | Strain Guage | | |
| Rejection | Air Jet / Flapper / Pusher / Falling Drop (Option) | | |
| Operation | Touch Screen | | |
| Alarm | Buzzer & Lamp | | |
| Check Range | 3-100g | 10-1200g | 30-3000g |
| Accuracy | +-0.1 | +-0.5 | -1 |
| Check Speed(Max) | 60 bags/min | 150 bags/min | 100 bags/min |
| Belt Speed | 30 m/min | 13-96 m/min | 13-70 m/min |
| Package length | 10-130mm | 60-300mm | 60-350mm |
| Package Width | 10-130mm | 20-200mm | 30-250mm |
| Package Height | 10-130mm | 10-200mm | 10-330mm |
| Weight Size | 300x130mm | 400x220mm | 500x300mm |
| Power | AC110V/220V 50-60HZ | | |
| Rated Output | Appr.200W | | |
| Dimension | 1468mm(L)\*558mm(W)\*1285±35mm(H) | | |